Hello all, first, thanks for this great group about a great simulator.  I seem to be having trouble with the CMOS chip.  Once that would function, I would plan to check to see if the voltage SW works also.

I observed almost a constant 5ma draw on the output side of the real (physical) chip.  In the simulation circuit, I am trying to get turn-on at about 4.8ma through the emitter diode and turn off when the current drops about 10%, or at about 4.3ma.  Or should the hysteresis involve more like a 5% current drop or so? 