Transient analysis of full wave rectifier that calculates input impedance at the fundamental frequency as a function of input voltage. Unzip into empty folder and run Full-wave_rectifier.asc. After running the analysis, view the error log and then plot step'ed data. Modified to include the 1N4007 model and harmonic current ratio in power factor calculation. 